For 1D buoy sim:

Calculate drag force that acts opposite to the sign of the difference between the buoy velocity and the wave velocity.

Where:

fluid density

difference between buoy velocity and wave velocity

skin-friction frag coefficient:

Where:

bluff-body drag coefficient, selected as 0.5

wetted area (surface area submerged in water)

reference area (cross-sectional area of buoy)